[Contents] [Prev] [Next] [Index] [Report an Error]

# atm bulk-config

#### Syntax

atm bulk-config bulkConfigName [ vc-range vpiStart vpiEnd vciStart vciEnd ]*

no atm bulk-config bulkConfigName [ vc-range vpiStart vpiEnd vciStart vciEnd ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures a range of ATM PVCs for use by a dynamic ATM 1483 subinterface, and assigns a name to the virtual circuit (VC) range. Each VC range consists of one or more nonoverlapping VC subranges. A VC subrange is a group of VCs that resides within the specified VPI and VCI ranges. You can configure multiple VC ranges on an ATM AAL5 interface. The no version removes the specified VC range (including all subranges in the range) from the ATM AAL5 interface or the specified subrange from the VC range. The no version also removes any overriding profile assignments for ATM PVCs within the deleted VC range or VC subrange.

| Note: The total number of VCs configured with the atm bulk-config command cannot exceed the maximum ATM VC capacity of the line module you are using. For details about the ATM VC capacity of supported line modules, see JUNOSe Release Notes, Appendix A, System Maximums.

#### Options

- bulkConfigName—Name of the VC range; string of up to 80 characters
- vpiStart—Starting virtual path identifier (inclusive) of the VC subrange you are configuring
- vpiEnd—Ending virtual path identifier (inclusive) of the VC subrange you are configuring
- vciStart—Starting virtual circuit identifier (inclusive) of the VC subrange you are configuring
- vciEnd—Ending virtual circuit identifier (inclusive) of the VC subrange you are configuring
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]