[Contents] [Prev] [Next] [Index] [Report an Error]

# aaa subscriber limit per-port

#### Syntax

aaa subscriber limit per-port interfaceSpecifier limitValue

no aaa subscriber limit per-port interfaceSpecifier

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets the maximum number of active subscribers permitted on the specified port. The no version returns the limit to the default, 0 (zero).

#### Options

- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- limitValue—Maximum number of subscribers; default value is 0 (zero), which means there is no limit on the number of subscribers

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]