[Contents] [Prev] [Next] [Index] [Report an Error]

# mpls ldp vpls vpls-id

#### Syntax

mpls ldp vpls vplsName vpls-id vplsId

no mpls ldp vpls vplsName vpls-id

#### Release Information

Command introduced in JUNOSe Release 8.2.0.

#### Description

Configures the globally unique VPLS identifier of a VPLS instance that uses LDP as the signaling protocol. All VEs that participate in the same VPLS domain must use the same VPLS identifier. The VPLS identifier configured for a VPLS instance must not be the same as the PWid for Martini configurations for Ethernet layer 2 services over MPLS. The no version deletes the VPLS identifier from the VPLS instance.

The mpls ldp vpls vpls-id command is not valid for a VPLS instance that uses BGP as the signaling protocol. To configure a VPLS instance with BGP signaling, use the bridge vpls rd, bridge vpls route-target, bridge vpls site-name site-id, and bridge vpls site-range commands.

#### Options

- vplsName—Name of a VPLS instance created with the bridge vpls transport-virtual-router command
- vplsId—VPLS identifier for the VPLS instance, in the range 1–4294967295

#### Mode

Global Configuration

#### Related Topics

- Configuring LDP Signaling for VPLS in the JUNOSe BGP and MPLS Configuration Guide

[Contents] [Prev] [Next] [Index] [Report an Error]