[Contents] [Prev] [Next] [Index] [Report an Error]

# Creating Rate-Limit Profiles

Create rate-limit profiles with a rate based on percentage and a burst in milliseconds. The system creates a policy using these rate-limit profiles and then attaches them to different interfaces using different parameter values.

1. Create policy parameter refRlpRate.
   `
   host1(config)#policy-parameter refRlpRate reference-rate
   host1(config-policy-param-reference-rate)#reference-rate 100000
   host1(config-policy-param-reference-rate)#exit
   `
2. Create rate-limit profile rlpData.
   `
   host1(config)#ip rate-limit-profile rlpData
   host1(config-rate-limit-profile)#committed-rate refRlpRate percentage 10
   host1(config-rate-limit-profile)#committed-burst millisecond 100
   host1(config-rate-limit-profile)#peak-rate refRlpRate percentage 100
   host1(config-rate-limit-profile)#peak-burst millisecond 150
   host1(config-rate-limit-profile)#exit
   `
3. Create rate-limit profile rlpVoice.
   `
   host1(config)#ip rate-limit-profile rlpVoice
   host1(config-rate-limit-profile)#committed-rate 64000
   host1(config-rate-limit-profile)#committed-burst 100000
   host1(config-rate-limit-profile)#peak-rate refRlpRate percentage 100
   host1(config-rate-limit-profile)#peak-burst millisecond 150
   host1(config-rate-limit-profile)#exit
   `
4. Create rate-limit profile rlpVideo.
   `
   host1(config)#ip rate-limit-profile rlpVideo
   host1(config-rate-limit-profile)#committed-rate refRlpRate percentage 70
   host1(config-rate-limit-profile)#committed-burst millisecond 100
   host1(config-rate-limit-profile)#peak-rate refRlpRate percentage 100
   host1(config-rate-limit-profile)#peak-burst millisecond 150
   host1(config-rate-limit-profile)#exit
   `
5. Create the policy.
   `
   host1(config)#ip policy-list P
   host1(config-policy)#classifier-group data
   host1(config-policy-classifier-group)#rate-limit-profile rlpData
   host1(config-policy-classifier-group)#exit
   host1(config-policy)#classifier-group voice
   host1(config-policy-classifier-group)#rate-limit-profile rlpVoice
   host1(config-policy-classifier-group)#exit
   host1(config-policy)#classifier-group video
   host1(config-policy-classifier-group)#rate-limit-profile rlpVideo
   host1(config-policy-classifier-group)#exit
   host1(config-policy)#exit
   `
6. Attach IP Policy P at interface atm5/0.1.
   `
   host1(config)#interface atm 5/0.1
   host1(config-if)#ip policy-parameter reference-rate refRlpRate 1000000
   host1(config-if)#ip policy input P
   `
7. Attach IP Policy P at interface atm5/0.2 with merge.
   `
   host1(config)#interface atm 5/0.2
   host1(config-if)#ip policy input P stats enabled merge
   `
8. Display the policy list.

       host1#show policy-list

       Policy Table
       ------ -----
       IP Policy P
          Administrative state: enable
          Reference count:      1
          Classifier control list: data, precedence 100
             rate-limit-profile rlpData
          Classifier control list: voice, precedence 100
             rate-limit-profile rlpVoice
          Classifier control list: video, precedence 100
             rate-limit-profile rlpVideo

          Referenced by interfaces:
             ATM5/0.1 input policy, statistics disabled, virtual-router default
             ATM5/0.2 input policy, statistics enabled, virtual-router default

          Referenced by profiles:
             None

          Referenced by merge policies:
             None

9. Display the rate-limit profiles.

       host1#show rate-limit-profile

       Rate Limit Profile Table
       ---- ----- ------- -----
       IP Rate-Limit-Profile: rlpData
          Profile Type:                   two-rate
          Reference count:                1
          Committed rate:                 refRlpRate % 10
          Committed burst:                100 milliseconds
          Peak rate:                      refRlpRate % 100
          Peak burst:                     150 milliseconds
          Mask:                           255
          Committed rate action:          transmit
          Conformed rate action:          transmit
          Exceeded rate action:           drop

       IP Rate-Limit-Profile: rlpVoice
          Profile Type:                   two-rate
          Reference count:                1
          Committed rate:                 64000
          Committed burst:                100000
          Peak rate:                      refRlpRate % 100
          Peak burst:                     150 milliseconds
          Mask:                           255
          Committed rate action:          transmit
          Conformed rate action:          transmit
          Exceeded rate action:           drop

       IP Rate-Limit-Profile: rlpVideo
          Profile Type:                   two-rate
          Reference count:                1
          Committed rate:                 refRlpRate % 70
          Committed burst:                100 milliseconds
          Peak rate:                      refRlpRate % 100
          Peak burst:                     150 milliseconds
          Mask:                           255
          Committed rate action:          transmit
          Conformed rate action:          transmit
          Exceeded rate action:           drop

10. Display policy parameters. If a rate-limit profile uses this parameter twice then it increases the reference count by 2.

        host1#show policy-parameter brief
        Reference-rate refRlpRate: 100000, 6 references

               Display policy parameters
        host1#show policy-parameter
        Policy Parameter refRlpRate
            Type: reference-rate
            Rate: 100000
            Reference count: 6
            Referenced by interfaces: 1 references
              IP interface ATM5/0.1: 1000000

            Referenced by rate-limit profiles: 5 references
              rlpData
              rlpVoice
              rlpVideo

11. Display interface atm5/0.1.

        host1#show ip interface atm 5/0.1
        ATM5/0.1 line protocol Atm1483 is down, ip is down (ready)
          Network Protocols: IP
          Internet address is 1.1.1.1/255.255.255.255
          Broadcast address is 255.255.255.255
          Operational MTU = 0  Administrative MTU = 0
          Operational speed = 100000000 Administrative speed = 0
          Discontinuity Time = 0
          Router advertisement = disabled
          Proxy Arp = disabled
          Network Address Translation is disabled
          TCP MSS Adjustment = disabled
          Administrative debounce-time = disabled
          Operational debounce-time    = disabled
          Access routing = disabled
          Multipath mode = hashed
          Auto Configure = disabled
          Auto Detect = disabled
          Inactivity Timer = disabled

          In Received Packets 0, Bytes 0
            Unicast Packets 0, Bytes 0
            Multicast Packets 0, Bytes 0
          In Policed Packets 0, Bytes 0
          In Error Packets 0
          In Invalid Source Address Packets 0
          In Discarded Packets 0
          Out Forwarded Packets 0, Bytes 0
            Unicast Packets 0, Bytes 0
            Multicast Routed Packets 0, Bytes 0
          Out Scheduler Dropped Packets 0, Bytes 0
          Out Policed Packets 0, Bytes 0
          Out Discarded Packets 0

          IP policy input P
            Statistics are disabled

12. Display interface atm5/0.2.

        host1#show ip interface atm 5/0.2
        ATM5/0.2 line protocol Atm1483 is down, ip is down (ready)
          Network Protocols: IP
          Internet address is 2.2.2.2/255.255.255.255
          Broadcast address is 255.255.255.255
          Operational MTU = 0  Administrative MTU = 0
          Operational speed = 100000000  Administrative speed = 0
          Discontinuity Time = 0
          Router advertisement = disabled
          Proxy Arp = disabled
          Network Address Translation is disabled
          TCP MSS Adjustment = disabled
          Administrative debounce-time = disabled
          Operational debounce-time    = disabled
          Access routing = disabled
          Multipath mode = hashed
          Auto Configure = disabled
          Auto Detect = disabled
          Inactivity Timer = disabled

          In Received Packets 0, Bytes 0
            Unicast Packets 0, Bytes 0
            Multicast Packets 0, Bytes 0
          In Policed Packets 0, Bytes 0
          In Error Packets 0
          In Invalid Source Address Packets 0
          In Discarded Packets 0
          Out Forwarded Packets 0, Bytes 0
            Unicast Packets 0, Bytes 0
            Multicast Routed Packets 0, Bytes 0
          Out Scheduler Dropped Packets 0, Bytes 0
          Out Policed Packets 0, Bytes 0
          Out Discarded Packets 0

          IP policy input P
            classifier-group data entry 1
              0 packets, 0 bytes
              rate-limit-profile rlpData
                   committed rate: 10000 bps, committed burst: 125 bytes
                   peak Rate: 100000 bps, peak burst: 1875 bytes
                committed: 0 packets, 0 bytes, action: transmit
                conformed: 0 packets, 0 bytes, action: transmit
                exceeded:  0 packets, 0 bytes, action: drop
            classifier-group voice entry 1
              0 packets, 0 bytes
              rate-limit-profile rlpVoice
                   committed rate: 64000 bps, committed burst: 100000 bytes
                   peak Rate: 100000 bps, peak burst: 1875 bytes
                committed: 0 packets, 0 bytes, action: transmit
                conformed: 0 packets, 0 bytes, action: transmit
                exceeded:  0 packets, 0 bytes, action: drop
            classifier-group video entry 1
              0 packets, 0 bytes
              rate-limit-profile rlpVideo
                   committed rate: 70000 bps, committed burst: 875 bytes
                   peak Rate: 100000 bps, peak burst: 1875 bytes
                committed: 0 packets, 0 bytes, action: transmit
                conformed: 0 packets, 0 bytes, action: transmit
                exceeded:  0 packets, 0 bytes, action: drop

To configure a policy-parameter at an interface with the increase keyword:

1. Create policy list P2.
   `
   host1(config)#ip policy-list P2
   host1(config-policy)#classifier-group data2
   host1(config-policy-classifier-group)#rate-limit-profile rlpData
   host1(config-policy-classifier-group)#exit
   host1(config-policy)#exit
   `
2. Attach IP Policy P2 at interface atm5/0.2 with the merge keyword.
   `
   host1(config)#interface atm 5/0.2
   host1(config-If)#ip policy-parameter reference-rate refRlpRate 100000
   `

   This increases from 0.

   `
   host1(config)#ip policy-parameter reference-rate refRlpRate increase 100000
   `

   This increases from the existing 100000.

   `
   host1(config)#ip policy input P2 merge
   `
3. Verify the configuration.

       host1#show policy-parameter
       Policy Parameter refRlpRate
           Type: reference-rate
           Rate: 100000
           Reference count: 7
           Referenced by interfaces: 2 references
             IP interface ATM5/0.1: 1000000
             IP interface ATM5/0.2: 200000

           Referenced by rate-limit profiles: 5 references
             rlpData
             rlpVoice
             rlpVideo

[Contents] [Prev] [Next] [Index] [Report an Error]