[Contents] [Prev] [Next] [Index] [Report an Error]

# show atm ping

#### Syntax

show atm ping [atm interfaceSpecifier [ vpi vci ] ] [ filter ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Displays a summary of the results (number of ping cells sent, number of ping cells received, success rate) of the ping operation. These results are overwritten when a new ATM ping is invoked for the circuit. If you do not specify any of the options, the command shows ping entries for the entire router.

#### Options

- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- vpi—Virtual path identifier
- vci—Virtual circuit identifier
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

[Contents] [Prev] [Next] [Index] [Report an Error]