[Contents] [Prev] [Next] [Index] [Report an Error]

# Before You Configure MLFR

Before you begin configuring MLFR, you must configure the physical layer interfaces that will be aggregated by MLFR.

The procedures described in this chapter assume that a physical layer interface, such as a T1 or T3 interface, has been configured. For details about configuring physical layer interfaces, see the JUNOSe Physical Layer Configuration Guide.

[Contents] [Prev] [Next] [Index] [Report an Error]