[Contents] [Prev] [Next] [Index] [Report an Error]

# mdt-data-delay

#### Syntax

mdt-data-delay timeout

no mdt-data-delay

#### Release Information

Command introduced in JUNOSe Release 8.2.0.

#### Description

Configures a timeout before switching to data MDT. The no version returns to the default.

#### Options

- timeout—Timeout value measured in 0.1 seconds in the range 1-255 seconds; the default is 30

#### Mode

IP PIM Data MDT Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]