[Contents] [Prev] [Next] [Index] [Report an Error]

# frame-relay lmi-t391dte

#### Syntax

frame-relay lmi-t391dte seconds

no frame-relay lmi-t391dte

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets the link integrity verification polling timer (T391) on a DTE interface. The no version removes the current setting and sets the default.

#### Options

- seconds—Number in the range 5–30 seconds; specifies the interval in seconds between status inquiries issued by the DTE; default value is 10 seconds

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]