[Contents] [Prev] [Next] [Index] [Report an Error]

# ip ospf authentication message-digest

#### Syntax

[ no ] ip ospf authentication message-digest

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies that the authentication mode for the interface is MD5. The no version sets authentication for the interface to none, but leaves any configured MD5 key intact.

#### Mode

Interface Configuration, Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]