[Contents] [Prev] [Next] [Index] [Report an Error]

# auto-configure atm1483

#### Syntax

[ no ] auto-configure atm1483

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures the static ATM AAL5 interface to support autodetection of an ATM 1483 dynamic encapsulation type. The no version terminates autodetection of the ATM 1483 encapsulation type.

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]