[Contents] [Prev] [Next] [Index] [Report an Error]

# Multinetting and Ethernet

Ethernet interfaces, except for bridged Ethernet interfaces, support multinetting; that is, adding more than one IP address to an IP interface. If you want to add multiple IP addresses to a single IP interface, use the ip address command with the secondary keyword, which is described in the chapter Configuring IP in JUNOSe IP, IPv6, and IGP Configuration Guide.

[Contents] [Prev] [Next] [Index] [Report an Error]