[Contents] [Prev] [Next] [Index] [Report an Error]

# Using Unicast Routes for RPF

You can use the ip route-type command to specify that BGP routes should be available for RPF. Routes available for RPF appear in the multicast view of the routing table.

| Note: This command functions the same for both IPv4 and IPv6 multicast.

ipv6 route-type

- Use to specify that BGP routes are available only for unicast forwarding, only for multicast RPF checks, or for both.
- Use the show ipv6 rpf-routes command to view the routes available for RPF.
- By default, BGP routes are available both for unicast forwarding and multicast reverse-path forwarding checks.
- Example
  `
  host1(config)#router bgp
  host1(config-router)#ipv6 route-type multicast
  `
- There is no no version.
- See ipv6 route-type.

[Contents] [Prev] [Next] [Index] [Report an Error]