[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Configured and Operational Status of all Destinations

#### Purpose

Display summary of the configured and operational status of all L2TP destinations.

#### Action

To display a summary of the configured and operational status of all L2TP destinations.:

    host1#show l2tp destination summary
    Administrative status    enabled    drain      disabled
                             0          0          0
    Operational status       up         down       lower-down not-present
                             0          0          0          0

#### Meaning

Table 86 lists the show l2tp destination summary command output fields.

Table 86: show l2tp destination summary Output Fields

Field Name | Field Description
--- | ---
Administrative status | Administrative status of the L2TP destination: enabled—No restrictions on creation and operation of sessions and tunnels for this destination drain—Router will not create new sessions or tunnels for this destination disabled—Router disabled existing sessions and tunnels and will not create new sessions or tunnels for this destination
Operational status | Operational status of the L2TP destination: up—Destination is available for tunnels down—Destination is not available for tunnels lower-down—Underlying transport is unavailable; for example, you removed the virtual router not-present—Hardware supporting the destination is unavailable; for example, you removed a required line module

#### Related Topics

- show l2tp destination summary

[Contents] [Prev] [Next] [Index] [Report an Error]