[Contents] [Prev] [Next] [Index] [Report an Error]

# default-metric

#### Syntax

[ no ] default-metric metricValue [ interfaceType interfaceSpecifier ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures RIP to use this metric on redistributed routes on all subsequently created interfaces. The no version restores the default value, 0.

#### Options

- metricValue—Metric to apply to routes; in the range 1–16
- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers

#### Mode

Address Family Configuration, Router Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]