[Contents] [Prev] [Next] [Index] [Report an Error]

# transform

#### Syntax

transform transform0
[ transform1 [ transform2 [ transform3 [ transform4 [ transform5 ] ] ] ] ]

no transform

#### Release Information

Command introduced in JUNOSe Release 7.3.0.

#### Description

Specifies the eligible transforms for this profile for IPSec source address negotiations. You can specify up to six transform algorithms for this profile. The no version resets the transform to the default, esp-3des-sha1.

#### Options

- transform0 through transform5—AH or ESP transform

#### Mode

IPSec Tunnel Profile Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]