[Contents] [Prev] [Next] [Index] [Report an Error]

# memory

#### Syntax

[ no ] memory warning highUtilization abatedUtilization

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures memory warning parameters. When the router reaches the high memory utilization value, it sends warning messages. When memory usage falls to the abated memory utilization value, the router stops sending warning messages. The no version returns the memory warning parameters to the default values.

#### Options

- highUtilization—High memory utilization value; in the range 1–99; default value is 85
- abatedUtilization—Abated memory utilization value; in the range 1–99; default value is 75

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]