[Contents] [Prev] [Next] [Index] [Report an Error]

# override c2 byte

#### Syntax

[ no ] override c2 byte

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Overrides the default value of the Path Signal Label (C2) byte for SONET and SDH interfaces. The no version restores the default setting.

#### Mode

Controller Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]