[Contents] [Prev] [Next] [Index] [Report an Error]

# vlan id

#### Syntax

vlan id idValue [ untagged ] [ mac-address macAddress ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies a VLAN ID. There is no no version.

#### Options

- idValue—Number unique within the Ethernet interface, in the range 0–4095
- untagged—Specifies that frames be sent untagged; valid only for VLAN ID 0
- macAddress—MAC address of the interface; when you do not specify a unique MAC address, the VLAN uses the MAC address of the Ethernet interface

#### Mode

Interface Configuration

#### Related Topics

- Configuring Ethernet/VLAN Layer 2 Services, Configuring Local ATM Cross-Connect with AAL5 Encapsulation, and Configuring Local Cross-Connects Between Ethernet/VLAN Interfaces in the JUNOSe BGP and MPLS Configuration Guide

[Contents] [Prev] [Next] [Index] [Report an Error]