[Contents] [Prev] [Next] [Index] [Report an Error]

# atm ilmi-keepalive

#### Syntax

[ no ] atm ilmi-keepalive [ seconds ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Enables generation of ILMI keepalive messages on the router, affecting the operational state of the ATM interface. The no version disables the generation of keepalive messages.

#### Options

- seconds—Number in the range 0–4294967295; the interval in seconds between two consecutive ILMI keepalive requests

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]