[Contents] [Prev] [Next] [Index] [Report an Error]

# load-interval

#### Syntax

load-interval timeInterval

no load-interval

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Sets the time interval at which the router calculates bit rates and packet rates for an interface. The no version restores the default value, 300 seconds. This command is not available for the Ethernet interface on the SRP module.

#### Options

- timeInterval—Multiple of 30 seconds; in the range 30–300

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]