[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring LDP

Purpose

Display information about LDP.

Action

To display LDP information:

    host1#show ldp
    LDP
      LSR ID is 80.0.0.2
      FEC Deaggregation is off
      Egress label: implicit-null
      Label distribution control mode: ordered control
      LDP session retry  0 times at interval 10
      LDP session hold time: 180
      LDP session keepalive interval: 20
      LDP targeted-hello hold time: 45
      LDP targeted-hello interval: 15
      Topology Driven LSP enabled
      LSPs used for IP forwarding
          for host addresses only

| Note: The mpls keyword is optional and is provided for compatibility with non–E-series implementations.

Meaning

Table 33 lists the show ldp command output fields.

Table 33: show ldp Output Fields

Field Name | Field Description
--- | ---
LSR ID | IP address of label-switched router
FEC Deaggregation | State of FEC deaggregation, on or off
Egress label | Type of label advertised for the LSR that is the egress router for the prefix, implicit null, explicit null, or a non-null label
Label distribution control mode | Label distribution control mode used by LDP for label distribution, independent control, or ordered control
LDP session retry | Configured values for the number of LDP session retry attempts and the retry interval
LDP session hold time | Configured value for the LDP session hold time
LDP session keepalive interval | Interval at which LDP sends session keepalive messages, in seconds
LDP targeted-hello hold time | LDP targeted-hello hold time, in seconds
LDP targeted-hello interval | LDP targeted-hello interval, in seconds
Topology Driven LSP | Status of topology-driven LSP, enabled or disabled
LSPs used for IP forwarding | LSPs are placed in the IP routing table for forwarding plain IP traffic; displayed only when the mpls ldp ip-forwarding command has been configured. Indicates whether the LSPs that are used for IP forwarding are host only, subject to a specified access list, or subject to a specified prefix list.
LDP proto stats | LDP protocol statistics
totalPeersDiscovered | Number of LDP peers discovered
totalAdjacenciesEstablished | Number of LDP adjacencies established
totalSessionsEstablished | Number of LDP sessions established
totalFECElements | Number of FEC elements
totalFECs | Number of FECs
totalInLabels | Number of in labels (sent to upstream neighbor)
totalOutLabels | Number of out labels (received from downstream neighbor)
totalCrLSPSetup | Number of constraint-based routed LSPs set up
totalCrLSPDeleted | Number of constraint-based routed LSPs deleted

#### Related Topics

- show ldp

[Contents] [Prev] [Next] [Index] [Report an Error]