[Contents] [Prev] [Next] [Index] [Report an Error]

# minimum-dynamic-rate-percent

#### Syntax

minimum-dynamic-rate-percent minimumDynamicRatePercent

no minimum-dynamic-rate-percent

#### Release Information

Command introduced in JUNOSe Release 8.0.0.

#### Description

Specifies the minimum value of the dynamic shaping rate as a percentage of the shared shaping rate for all simple shared shapers on the router. The no version removes the specified minimum dynamic rate from all simple shared shapers on the router.

#### Options

- minimumDynamicRatePercent—Minimum percentage value of the dynamic shared shaper in the range 0–100; default value is 0

#### Mode

QoS Shared Shaper Control Configuration

#### Related Topics

- Configuring Simple Shared Shaper Algorithm Variables

[Contents] [Prev] [Next] [Index] [Report an Error]