[Contents] [Prev] [Next] [Index] [Report an Error]

# radius nas-port-format

#### Syntax

radius nas-port-format { 0ssssppp | ssss0ppp }

no radius nas-port-format

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures the RADIUS client’s use of a specific format for RADIUS attribute 5, NAS-Port. The no version removes the format.

#### Options

- 0ssssppp—Sets the RADIUS client to use the 0ssssppp format where s is slot and p is port
- ssss0ppp—Sets the RADIUS client to use the ssss0ppp format where s is slot and p is port

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]