[Contents] [Prev] [Next] [Index] [Report an Error]

# cablelength

#### Syntax

cablelength length

no cablelength

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the length of the cable, which determines power requirements. The no version uses the default value, 0 feet.

#### Options

- length —Cable length in the range 0–450 feet

#### Mode

Controller Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]