[Contents] [Prev] [Next] [Index] [Report an Error]

# baseline mpls interface

#### Syntax

baseline mpls interface interfaceName

#### Release Information

Command introduced in JUNOSe Release 7.1.0.

#### Description

Sets a statistics baseline for the specified MPLS major interface or MPLS shim interface. By default, the interface counters are baselined at zero. There is no no version.

#### Options

- interfaceName—Name of interface; up to 15 alphanumeric characters

#### Mode

Privileged Exec

#### Related Topics

- Setting Baselines for Layer 2 Services over MPLS in the JUNOSe BGP and MPLS Configuration Guide

[Contents] [Prev] [Next] [Index] [Report an Error]