[Contents] [Prev] [Next] [Index] [Report an Error]

# aps lockout

#### Syntax

aps lockout [ 0 ]

no aps lockout

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Prevents the working interface from switching to the protect interface. The no version restores the default situation, in which the working interface can switch to the protect interface.

#### Options

- 0—Specifies the channel number that identifies the protect interface; because the protect interface is always assigned channel number 0, this is the only valid option

#### Mode

Controller Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]