[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring Bridging-Related Settings for VPLS

You can use the show commands listed in Table 83 to display VPLS settings related to transparent bridging. Except for the show bridge interface vpls command, which is only for VPLS instances, you can use these commands to monitor both VPLS instances and standard bridge groups for transparent bridging.

Table 83: Commands for Monitoring VPLS Bridging Settings

show bridge | show bridge port
show bridge groups | show bridge table
show bridge interface | show subscriber-policy
show bridge interface vpls |

#### Related Topics

- Monitoring VPLS Configuration and Statistics for a Specific VPLS Instance
- Monitoring VPLS Configuration and Statistics for all VPLS Instances
- Monitoring Configuration, Statistics, and Status for VPLS Network Interfaces
- Monitoring Configuration, Statistics, and Status for VPLS Core Interfaces
- Monitoring Configuration, Statistics, and Status for VPLS Ports
- Monitoring MAC Address Entries for a Specific VPLS Instance
- Monitoring Subscriber Policy Rules
- For more information about using these commands, see Monitoring Transparent Bridging in the JUNOSe Link Layer Configuration Guide.

[Contents] [Prev] [Next] [Index] [Report an Error]