[Contents] [Prev] [Next] [Index] [Report an Error]

# interface-event-disable

#### Syntax

[ no ] interface-event-disable

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies that RIP does not purge the routing table on a RIP interface that has been brought down. The no version restores the default condition, wherein RIP does purge the routing table on an interface after a down event.

#### Mode

Address Family Configuration, Router Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]