[Contents] [Prev] [Next] [Index] [Report an Error]

# radius override nas-port-id remote-circuit-id

#### Syntax

radius override nas-port-id remote-circuit-id

no radius override nas-port-id

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures RADIUS to override the standard use of the NAS-Port-Id [87] RADIUS attribute and instead use the PPPoE remote circuit ID transmitted from a DSLAM device. The no version restores the default NAS-Port-Id value, which is the physical interface of the network access server (NAS) that is authenticating the user.

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]