[Contents] [Prev] [Next] [Index] [Report an Error]

# isis lsp-interval

#### Syntax

isis lsp-interval milliseconds

no isis lsp-interval

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures the time delay between successive IS-IS link-state packet transmissions. The no version restores the default value, 33 milliseconds.

#### Options

- milliseconds—Number of milliseconds in the range 1–4294967295; an interval between successive link-state packets

#### Mode

Interface Configuration, Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]