> - Download PDFs
> - radius vlan nas-port-format stacked

> # radius vlan nas-port-format stacked

> #### Syntax

> radius vlan nas-port-format stacked

> no radius vlan nas-port-format

> #### Release Information

> Command introduced before JUNOSe Release 7.1.0.

> #### Description

> Configures the RADIUS NAS-Port attribute to include the S-VLAN ID, in addition to the VLAN ID, for subscribers on Ethernet interfaces. The no version restores the default situation, which does not include the S-VLAN ID.

> #### Mode

> Global Configuration

> #### Updated: 2009-04-17

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.