[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring QoS for Tunnel-Server Ports for L2TP LNS Sessions

You can configure QoS for a tunnel-service port that can be used as a dynamic interface associated with an L2TP LNS session.

Before you configure QoS for a tunnel-server port:

- Configure the dedicated or shared tunnel-server port.

  See JUNOSe Physical Layer Configuration Guide.

- Configure the traffic classes.

  See Configuring Traffic Classes That Define Service Levels.

- Configure the queuing hierarchy.

  See Configuring Queue Profiles to Manage Buffers and Thresholds.

- Configure the scheduler hierarchy and shaping with scheduler profiles.

  See Configuring a Scheduler Hierarchy.

To configure QoS for the tunnel-server port:

1. Create the QoS profile.
   `
   host1(config)#qos-profile lns-tsport
   `
2. Configure group nodes for the tunnel-server ports.
   `
   host1(config-qos-profile)#ip queue traffic-class best-effort scheduler-profile business-data queue-profile data
   host1(config-qos-profile)#ip queue traffic-class video scheduler-profile video queue-profile video
   host1(config-qos-profile)#ip queue traffic-class voice scheduler-profile voice queue-profile voice
   host1(config-qos-profile)#server-port group video
   host1(config-qos-profile)#server-port group data
   host1(config-qos-profile)#server-port group voice scheduler-profile strict-priority
   `
3. Create and attach the QoS port-type profile for server ports.
   `
   host1(config)#qos-port-type-profile server-port qos-profile lns-tsport
   `

#### Related Topics

- For more information about tunnel-server ports, see JUNOSe Physical Layer Configuration Guide
- group command
- interface command
- node command
- qos-port-type-profile command
- qos-profile command
- queue command
- scheduler-profile command
- traffic-class command
- tunnel-server command

[Contents] [Prev] [Next] [Index] [Report an Error]