[Contents] [Prev] [Next] [Index] [Report an Error]

# mpls atm vpi range

#### Syntax

mpls atm vpi range minVPI maxVPI

no mpls atm vpi range

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the range for virtual path identifiers that can be used in MPLS labels for an MPLS major interface on an ATM AAL5 interface using the interface label space. Creates the MPLS major interface if it does not yet exist. An error message is generated if you issue the command for any other layer 2 interface, as they do not support the interface label space. The no version deletes the range.

#### Options

- minVPI—Lowest virtual path identifier acceptable for a label, a value in the range 0–255
- maxVPI—Highest virtual path identifier acceptable for a label, a value in the range 0–255

#### Mode

Interface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]