[Contents] [Prev] [Next] [Index] [Report an Error]

# atm atm1483 subscriber

#### Syntax

atm atm1483 subscriber upperInterfaceType { user | user-prefix } userName
domain domainName [ { password | password-prefix }
password ] [ no-authenticate ]

no atm atm1483 subscriber upperInterfaceType

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures a local subscriber (when one cannot be obtained externally, as in PPP) for a dynamic upper interface encapsulation type configured over a dynamic ATM 1483 subinterface. A subscriber supports authentication and configuration from the RADIUS server. The no version removes the subscriber.

#### Options

- upperInterfaceType—One of the following dynamic encapsulation types:
  - bridgedEthernet
  - ip
- user—Employs the username as specified
- user-prefix—Appends the interface physical location to the username
- userName—RADIUS username
- domainName—Domain name
- password—Employs the password as specified
- password-prefix—Appends the interface physical location to the password
- password—RADIUS password
- no-authenticate—Disables authentication

#### Mode

Profile Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]