[Contents] [Prev] [Next] [Index] [Report an Error]

# ip split-horizon

#### Syntax

[ no ] ip split-horizon

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Enables split horizon, preventing the RIP router from advertising routes from the interface originating the route, reducing the possibility of routing loops; this is the default condition. The no version disables split horizon.

#### Mode

Interface Configuration, Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]