[Contents] [Prev] [Next] [Index] [Report an Error]

# radius override nas-info

#### Syntax

[ no ] radius override nas-info

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Configures the RADIUS client for a virtual router context to override the standard use of the NAS-IP-Address [4] and NAS-Identifier [32] attributes when the client performs AAA broadcast accounting. Normally, AAA accounting packets include the NAS-IP-Address and NAS-Identifier attributes of the virtual router that generates the accounting information. However, this command specifies that the broadcast accounting packets instead include the authenticating virtual router’s NAS-IP-Address and NAS-Identifier attributes. The no version restores the standard use of the two attributes in AAA accounting information.

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]