[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring the Routing Table

#### Purpose

Display the current state of the routing table, including routes not used for forwarding. An Access-P entry in the Type column of the output indicates routes that are downloaded by the RADIUS route-download server.

#### Action

To display information in the routing table:

    host1#show ip route
    Protocol/Route type codes:
      I1- ISIS level 1, I2- ISIS level2,
      I- route type intra, IA- route type inter, E- route type external,
      i- metric type internal, e- metric type external,
      P- periodic download, O- OSPF, E1- external type 1, E2- external type2,
      N1- NSSA external type1, N2- NSSA external type2
      L- MPLS label, V- VRF, *- via indirect next-hop

    Prefix/Length      Type       Next Hop      Dst/Met          Interface
    ------------------ --------- --------------- ---------- -----------------
    0.0.0.0/0          Static    10.13.10.1      1/0        FastEthernet6/0/0
    192.168.10.0/23    Connect   10.13.10.187    0/0        FastEthernet6/0/0
    192.168.21.21/32   Access-P  255.255.255.255 254/2      null0
    192.168.22.22/32   Access-P  255.255.255.255 254/2      null0
    192.168.23.23/32   Access-P  255.255.255.255 254/2      null0
    192.168.24.24/32   Access-P  255.255.255.255 254/2      null0

#### Meaning

Refer to the description of the show ip route command in JUNOSe IP, IPv6, and IGP Configuration Guide for additional information about the show ip route command.

#### Related Topics

- show ip route

[Contents] [Prev] [Next] [Index] [Report an Error]