> - Download PDFs
> - ipv6 initial-sequence-preference

> # ipv6 initial-sequence-preference

> #### Syntax

> ipv6 initial-sequence-preference preference

> no ipv6 initial-sequence-preference

> #### Release Information

> Command introduced in JUNOSe Release 9.3.0.

> #### Description

> Configures the warm restart replay preference for an IPv6 interface after a high availability switchover. The no version restores the default value.

> #### Options

> - preference—Preference value, 0 or 1; 1 indicates highest preference; default value is 0

> #### Mode

> Subinterface Configuration

> #### Updated: 2009-04-22

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.