[Contents] [Prev] [Next] [Index] [Report an Error]

# receive-interface

#### Syntax

receive-interface interfaceType interfaceSpecifier

no receive-interface

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the interface on which the RTR probe expects to receive responses. You must set this attribute when multiple RTR entries are configured to use the same target address. Specifying a receiving interface enables the router to map incoming RTR responses to the proper RTR entry, even when multiple RTR entries have the same target address. The no version restores the default value, which is to receive a response on any interface.

#### Options

- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers

#### Mode

RTR Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]