[Contents] [Prev] [Next] [Index] [Report an Error]

# mount

#### Syntax

mount { disk0 | disk1 }

no mount { disk0 | disk1 } [ force ]

#### Release Information

Command introduced in JUNOSe Release 8.0.0.

#### Description

Mounts the specified flash card. If the card was not safely unmounted previously, the command also performs disk and file system integrity checks before mounting the card and permitting user access. The no version prepares the card for safe unmounting by rejecting requests to open files and waiting for currently open files to close; only then is the user notified that the unmounted card can be safely ejected.

#### Options

- disk0—Specifies flash card in slot 0 of the SRP module; although this option is displayed by the CLI, it is rejected when specified because disk0 is required for router operation
- disk1—Specifies flash card in slot 1 of the SRP module; supported only on the E120 router and the E320 router
- force—Forces the dismount even when files on the disk are open for modification

#### Mode

Privileged Exec

[Contents] [Prev] [Next] [Index] [Report an Error]