[Contents] [Prev] [Next] [Index] [Report an Error]

# flash-disk initialize

#### Syntax

flash-disk initialize [ no-format ] [ disk0 | disk1 ]

#### Release Information

Command introduced before JUNOSe Release 7.1.0.
disk0 and disk1 keywords added in JUNOSe Release 7.2.0.
Privileged Exec mode added in JUNOSe Release 8.0.0.

#### Description

Performs a low-level format of unmounted flash cards. There is no no version.

#### Options

- no-format—Erases all files but does not format the flash card
- disk0—Specifies flash card in slot 0 of the SRP module; default value is disk0; available only in Boot mode, because disk0 cannot be in an unmounted state in a router outside of Boot mode
- disk1—Specifies flash card in slot 1 of the SRP module; supported only on the E120 router and the E320 router

#### Mode

Boot, Privileged Exec

[Contents] [Prev] [Next] [Index] [Report an Error]