[Contents] [Prev] [Next] [Index] [Report an Error]

# Monitoring the Delimiter Character in the Remote-Circuit-ID for RADIUS

#### Purpose

Display the delimiter character configured to set off components in the PPPoE remote circuit ID value captured from a DSLAM. The default delimiter character is #.

#### Action

To display the delimiter character:

    host1#show radius remote-circuit-id-delimiter
    !

#### Related Topics

- show radius remote-circuit-id-delimiter

[Contents] [Prev] [Next] [Index] [Report an Error]