[Contents] [Prev] [Next] [Index] [Report an Error]

# ip tunnel reassembly

#### Syntax

[ no ] ip tunnel reassembly

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Enables the reassembly of fragmented IP tunnel packets that are received on the current virtual router. The no version restores the default disabled condition.

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]