[Contents] [Prev] [Next] [Index] [Report an Error]

## ipGeneral

#### Description

IP general

#### Emergency

None

#### Alert

None

#### Critical

(IP) Interface stacking management errors

#### Error

(ARP) Allocation of Ethernet next hop failed
(IP) Not able to create interface or create address on null 0 interface; undefined IP status code; interface stacking management errors; send and forward failures because of not finding corresponding egress or ingress nodes; conflict in adding hidden routes

#### Warning Log

(IP) NVS load errors; failure to add address on an interface because of low memory

#### Notice Log

None

#### Info

None

#### Debug

(ARP) NextHopPool is out of memory and trying to expire old entries; ARP data events
(IP) Interface stacking management errors

#### Filter 1

interface interfaceType interfaceSpecifier

- interface—Logs events for a specific interface
- interfaceType—Type of interface for which you want to log events
- interfaceSpecifier—Location of interface in the appropriate format

  | Note: For information about interface types and specifiers, see Interface Types and Specifiers in JUNOSe Command Reference Guide.

#### Filter 2

router virtualRouterName [ interface interfaceType interfaceSpecifier ]

- router—Logs events for a specific virtual router
- virtualRouterName—Name of virtual router for which you want to log events
- interface—Logs events on a specific interface on the virtual router
- interfaceType—Type of interface for which you want to log events. For example, atm or fastEthernet.
- interfaceSpecifier—Location of interface in the appropriate format

  | Note: For information about interface types and specifiers, see Interface Types and Specifiers in JUNOSe Command Reference Guide.

[Contents] [Prev] [Next] [Index] [Report an Error]