[Contents] [Prev] [Next] [Index] [Report an Error]

# bandwidth

#### Syntax

bandwidth bandwidth

no bandwidth

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the total bandwidth available on the interface. The no version removes the admission control configuration from the interface. For total reservable bandwidth, see the mpls bandwidth command.

#### Options

- bandwidth—Available bandwidth in kilobits per second, a value from 1–10,000,000

#### Mode

Interface Configuration, Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]