[Contents] [Prev] [Next] [Index] [Report an Error]

# show radius remote-circuit-id-delimiter

#### Syntax

show radius remote-circuit-id-delimiter

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Displays the delimiter character that the router uses to set off components in the PPPoE remote circuit ID value sent from a DSLAM and captured on the router. The default delimiter character is #.

#### Mode

Privileged Exec

[Contents] [Prev] [Next] [Index] [Report an Error]