[Contents] [Prev] [Next] [Index] [Report an Error]

# pppoe sessions

#### Syntax

pppoe sessions sessions

no pppoe sessions

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Specifies the number of subinterfaces permitted on a PPPoE interface. The command affects only subinterfaces that are created after the command is entered. Previously created interfaces remain, even if their number exceeds the new value of the parameter. The no version restores the default value, 8000 (ERX routers) and 16,000 (E120 and E320 routers).

#### Options

- sessions—Number of subinterfaces permitted on the interface in the range 1–8000 (ERX routers) or 1–16,000 (E120 and E320 routers); default value is 8000 (ERX routers) or 16,000 (E120 and E320 routers)

#### Mode

Interface Configuration, Profile Configuration, Subinterface Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]