[Contents] [Prev] [Next] [Index] [Report an Error]

# igmp promiscuous

#### Syntax

[ no ] igmp promiscuous

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Allows all IGMP interfaces on the router to accept IGMP reports from hosts on any subnet. The no version allows IGMP interfaces on the router to accept IGMP reports only from hosts on their associated subnets.

#### Mode

Router Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]