[Contents] [Prev] [Next] [Index] [Report an Error]

# ip pim ssm

#### Syntax

ip pim ssm [ default | range ipAccessList ]

no ip pim ssm

#### Release Information

Command introduced before JUNOSe Release 7.1.0.

#### Description

Enables SSM and defines the SSM range of IP multicast addresses. The no version disables SSM on the router.

#### Options

- default—Specifies that SSM use the IANA-specified range of 232/8
- ipAccessList—Name of the IP access list that specifies the range of multicast addresses you want SSM to use

#### Mode

Global Configuration

[Contents] [Prev] [Next] [Index] [Report an Error]