[Contents] [Prev] [Next] [Index] [Report an Error]

# Transporting Packets Across an IP Backbone with MPLS

As described in the previous section, PE 1 and PE 2 exchange routing information, including MPLS labels for their customer sites, by means of a BGP session established between them across the service provider core.

| Note: To better understand MPLS before you read this section, see Configuring MPLS.

Labels are employed in both the BGP control plane and the MPLS data plane. In the control plane, BGP advertises a route with an in label; this in label is also the label needed when MPLS traffic is received. BGP receives routes with an associated out label; the out label is the label sent with MPLS traffic.

Consider the network shown in Figure 73. If you display the in label on PE 1, you see that MP-BGP advertises a labeled VPN-IPv4 prefix of 10.12.0.0/16 with an in label of 24 (and an RD of 777:1, as shown in the illustration).

    host1:pe1#show ip bgp vpn all field in-label
    Prefix         In-label
    10.12.0.0/16     24
    10.24.0.0/16     none

Figure 73: BGP/MPLS VPN Route Exchange

If you display the in label on PE 2, you see that MP-BGP advertises a labeled VPN-IPv4 prefix of 10.24.0.0/16 with an in label of 16 (and an RD of 777:5, as shown in the illustration).

    host2:pe2#show ip bgp vpn all field in-label
    Prefix         In-label
    10.12.0.0/16     none
    10.24.0.0/16     16

On PE 1, you see that MP-BGP receives a labeled VPN-IPv4 prefix of 10.24.0.0/16 with an out label of 16. MP-BGP on PE 2 advertised this label with the prefix. In the data plane, MPLS traffic is sent by PE 1 to PE 2 with this label.

    host1:pe1#show ip bgp vpn all field out-label
    Prefix         Out-label
    10.12.0.0/16     none
    10.24.0.0/16     16

On PE 2, you see that MP-BGP receives a labeled VPN-IPv4 prefix of 10.12.0.0/16 with an out label of 24. MP-BGP on PE 1 advertised this label with the prefix. In the data plane, MPLS traffic is sent by PE 2 to PE 1 with this label.

    host2:pe2#show ip bgp vpn all field out-label
    Prefix         Out-label
    10.12.0.0/16     24
    10.24.0.0/16     none

The data packets are transported within a VPN across the service provider core by MPLS. This transport process requires two layers of MPLS labels, stacked one upon the other.

The inner labels are assigned by each PE router for each VRF. When an MPLS packet arrives at the egress PE router, that egress PE router uses the inner label to determine which VRF the packet is destined for. In the default, per-VRF label allocation mode (described in Creating Labels per FEC), the egress PE router does an IP lookup in the IP forwarding table of that VRF using the IP destination address in the IP packet that is encapsulated in the MPLS packet. The egress PE router then forwards the IP packet (without the MPLS header) to the appropriate customer site. The inner labels themselves are communicated between PE routers in the MP-BGP extended update messages as described in the previous section.

MPLS uses the outer labels to forward data packets from the ingress PE router through a succession of P routers across the core. This succession of P routers constitutes a label-switched path (LSP), also referred to as an MPLS tunnel. The labels are assigned to links in the path.

At each P router, MPLS pops the outer label from a data packet. The label is an index into the P router’s forwarding table, from which it determines both the next hop along the LSP and another label. The router pushes the label on to the label stack and forwards the packet to the next P router. The combination of popping one label and pushing another is known as a label swap. At the egress PE router, MPLS pops the outer label, then the inner label. The inner label determines the CE router to which the packet is sent. The P routers never examine the inner MPLS label or the destination IP address encapsulated in the MPLS packet.

In many cases, the PE routers are fully meshed by means of LSPs. You can use tunnel profiles to simplify the LSP configuration process. See Configuring MPLS, for procedures to configure an LSP.

Each LSP is unidirectional for data traffic, so you must establish LSPs in both directions for two-way data transport. Figure 74 shows that two LSPs have been created between PE 1 and PE 2. PE 1 and PE 2 have an MP-BGP session as shown previously in Figure 73.

Figure 74: LSP Creation for BGP/MPLS VPN

The PE 1–PE 2 LSP carries traffic only from PE 1 to PE 2, using label 21 for the PE 1 to P 1 link, label 19 for the P 1 to P 2 link, and label 46 for the P 2 to PE 2 link. PE 1 can forward data packets along the LSP to PE 2 and its customer sites.

Similarly, the PE 2–PE 1 LSP carries traffic only from PE 2 to PE 1, using label 58 for the PE 2 to P 2 link, label 12 for the P 2 to P 1 link, and label 37 for the P 1 to PE 1 link. PE 2 can forward data packets along the LSP to PE 1 and its customer sites.

Example: Data Transport

The process of data transport is shown in Figure 75. PE 1 has already received announcements from PE 2; an LSP has been established between PE 1 and PE 2.

Figure 75: Traffic Across the MPLS Backbone of a BGP/MPLS VPN

Host 1 constructs an IP packet with the address of Host 2 as the final destination, and sends the packet to router CE 1. CE 1 encapsulates the packet appropriately and forwards it to PE 1.

PE 1 receives the packet from CE 1. Based on the interface the packet came in on, PE 1 determines that it must use the forwarding table for VRF A to route the packet. PE 1 looks up the destination address of Host 2 in the forwarding table of VRF A and finds the following instructions:

- Push label 16; that is, prepend it to the data packet. This innermost label identifies the VRF on PE 2, where the final destination and interface lookup takes place. Label 16 was previously allocated by PE 2 and communicated to PE 1 by MP-BGP. VRF A shows this label as part of the NLRI for destination address Host 2.
- Push label 21 and forward the MPLS-encapsulated data packet to router P 1. Label 21 is prepended to label 16; the labels are stacked. Label 21 becomes the outermost label and is assigned to the first segment—PE 1–P 1—in the label-switched path from PE 1 to PE 2. The LSP was previously configured.

P 1 receives the data packet from PE 1 and pops label 21. P 1 looks up label 21 in its forwarding table and determines it must push label 19 on the stack, and forwards the data packet to P 2.

P 2 receives the data packet from P 1 and pops label 19. P 2 looks up label 19 in its forwarding table and determines it must push label 46 on the stack, and forwards the data packet to PE 2.

PE 2 receives the data packet from P 2, and looks up label 46. PE 2 determines it is the egress router of the LSP and must pop label 46. Then it proceeds to look up the next label, label 16, and determines that the packet goes to VRF A. Then the IP address is looked up in VRF A to determine the destination and outgoing interface for the packet. PE 2 forwards the packet to CE 6.

CE 6 receives the IP packet from PE 2 and looks up the destination address Host 2. Subsequent forwarding to Host 2 occurs by means of the IGP in the customer site.

The network structure shown in Figure 75 consists of two VPNs, A and B. VPN A comprises CE 1, CE 5, and CE 6. VPN B comprises CE 2, CE 3, and CE 4. CE 1 has data traffic destined for both CE 5 and CE 6. Because both of these destination sites are within the same VPN, PE 1 uses the same forwarding table, in VRF A, to do the lookups and MPLS encapsulation. The innermost label determines the destination VRF and is the same for all packets in that VPN, even if they are destined for different CE routers. CE 2 and CE 3 have traffic destined for CE 4. Because these all are in VPN B, PE 1 uses a different forwarding table, in VRF B, for looking up destinations for traffic originating with these sites. However, both VPNs use the same LSP, because both VPNs use the same ingress (PE 1) to and the same egress (PE 2) from the service provider core. Remember that the illustrated LSP carries data traffic only from PE 1 to PE 2. Traffic from PE 2 to PE 1 requires a different LSP.

[Contents] [Prev] [Next] [Index] [Report an Error]